IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-12-23T14:28:11"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "ktemmerman" of Organization (no name given)
  Owner history of Person "ktemmerman" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1608728402 (2020-12-23T13:00:02Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 59 elements
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof_Recticel Insulation:88295" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          17 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standard" | object type "BERSfr_XX_GM_FB_logo_recticel:standard" | names: "BERSfr_XX_GM_FB_logo_recticel:standard:88311", "BERSfr_XX_GM_FB_logo_recticel:standard:88351", "BERSfr_XX_GM_FB_logo_recticel:standard:88390" (+14 more) | material: materials ("BERSnl_x_rgb 0 0 0 T00 noir_gen", "RSen_x_rgb 255 203 012 T00 yellow_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x100_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x100_Recticel Insulation:88335" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          25 x IFCBUILDINGELEMENTPROXY | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:88353", "Model Text:Model Text 1:88392", "Model Text:Model Text 1:88393" (+22 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x100_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x100_Recticel Insulation:88374" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x120_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x120_Recticel Insulation:88414" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x120_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x120_Recticel Insulation:88453" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x140_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x140_Recticel Insulation:88493" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x140_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x140_Recticel Insulation:88532" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x160_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x160_Recticel Insulation:88572" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x160_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x160_Recticel Insulation:88611" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x180_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x180_Recticel Insulation:88651" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x180_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x180_Recticel Insulation:88690" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x60_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x60_Recticel Insulation:88730" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x60_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x60_Recticel Insulation:88769" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x80_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x80_Recticel Insulation:88809" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x80_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x80_Recticel Insulation:88848" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x90_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 1200x1200x90_Recticel Insulation:88888" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x90_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Euroroof 2400x1200x90_Recticel Insulation:88927" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon

Types
  IFCBUILDINGELEMENTPROXYTYPE "standard" | 17 occurrences | material: materials ("BERSnl_x_rgb 0 0 0 T00 noir_gen", "RSen_x_rgb 255 203 012 T00 yellow_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Pset_ElementShading | properties | on 34 objects (17 IFCROOF, 17 IFCSLAB)
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 42 objects (42 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 34 objects (17 IFCROOF, 17 IFCSLAB)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 25 objects (25 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 17 objects (17 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x140_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 11 more contents on 22 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x140_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x140_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x160_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon: 9 more contents on 9 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x140_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x140_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x160_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 9 more contents on 9 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x140_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.157142857142857 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 2400x1200x140_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.157142857142857 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Euroroof 1200x1200x160_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.1375 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 9 more contents on 9 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 25 objects (25 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 17 objects (17 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standard" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)

Other addresses and roles
  2 x postal address (none given)