IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-12-23T14:15:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "ktemmerman" of Organization (no name given)
  Owner history of Person "ktemmerman" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1608728403 (2020-12-23T13:00:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 40 elements
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation:81118" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standaard" | object type "BERSnl_XX_GM_FB_logo_recticel:standaard" | names: "BERSnl_XX_GM_FB_logo_recticel:standaard:81134", "BERSnl_XX_GM_FB_logo_recticel:standaard:81173", "BERSnl_XX_GM_FB_logo_recticel:standaard:81213" (+8 more) | material: materials ("BERSnl_x_rgb 0 0 0 T00 zwart_gen", "BERSnl_x_rgb 255 203 012 T00 geel_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Other
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation:81157" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation:81197" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          18 x IFCBUILDINGELEMENTPROXY | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:81215", "Model Text:Model Text 1:81216", "Model Text:Model Text 1:81255" (+15 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions, Graphics
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation:81237" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation:81277" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation:81317" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x40/60_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x40/60_Recticel Insulation:81357" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x45/60_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x45/60_Recticel Insulation:81396" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x60/75_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x60/75_Recticel Insulation:81436" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x60/80_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x60/80_Recticel Insulation:81476" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction
          1 x IFCROOF | object type "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x75/90_Recticel Insulation" | names: "Basic Roof:BERSnl_27_RO_Eurothane Bi-4 A 1200x600x75/90_Recticel Insulation:81516" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon, Constraints, Construction

Types
  IFCBUILDINGELEMENTPROXYTYPE "standaard" | 11 occurrences | material: materials ("BERSnl_x_rgb 0 0 0 T00 zwart_gen", "BERSnl_x_rgb 255 203 012 T00 geel_gen") | property sets: Constraints, Identity Data, Materials and Finishes, Other, Pset_BuildingElementProxyCommon, Pset_ProductRequirements

Property sets
  Other(Type) | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Model Text" (IFCTEXT)
  Other(Type) | properties | on 11 objects (11 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family Name = "Basic Roof" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ElementShading | properties | on 22 objects (11 IFCROOF, 11 IFCSLAB)
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 29 objects (29 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 22 objects (11 IFCROOF, 11 IFCSLAB)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standaard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 5 more contents on 10 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x40/60_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x45/60_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon: 3 more contents on 3 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x40/60_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x45/60_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 3 more contents on 3 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.6 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.6 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.26 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.247619047619048 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.65 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.577777777777778 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x40/60_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.433333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x45/60_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.433333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 3 more contents on 3 objects not shown
  Constraints | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : Level 1" (IFCTEXT)
  Constraints | properties | on 11 objects (11 IFCROOF)
    Base Level = "Level: Level 1" (IFCLABEL)
    Base Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cutoff Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Roof : BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" (IFCTEXT)
  Constraints: 7 more contents on 6 objects not shown
  Construction | properties | on 2 objects (2 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 2 objects (2 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 105. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction: 1 more content on 1 objects not shown
  Dimensions | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Depth = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Area = 0.114476516316835 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000206579980456013 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.1124126784 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.6744760704 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.124126784 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 105. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.1803331232 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.4496507136 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.5058570528 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 4 more contents on 4 objects not shown
  Other | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Model Text: Model Text 1" (IFCLABEL)
    Family and Type = "Model Text: Model Text 1" (IFCLABEL)
    Type = "Model Text: Model Text 1" (IFCLABEL)
    Type Id = "Model Text: Model Text 1" (IFCLABEL)
  Other | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Family and Type = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
    Type Id = "BERSnl_XX_GM_FB_logo_recticel: standaard" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCLABEL)
    Family and Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCLABEL)
    Type = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCLABEL)
    Type Id = "Basic Roof: BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCLABEL)
  Other: 8 more contents on 7 objects not shown
  Phasing | properties | on 40 objects (29 IFCBUILDINGELEMENTPROXY, 11 IFCROOF)
    Phase Created = "New Construction" (IFCLABEL)
  Identity Data(Type) | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Model Text 1" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane Bi-4 A (1/60)_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane Bi-4 A (1/80)_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x80/100_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x90/105_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x20/40_Recticel Insulation" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "BERSnl_27_RO_Eurothane Bi-4 A 1200x600x30/45_Recticel Insulation" (IFCTEXT)
  Identity Data(Type): 5 more contents on 5 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standaard" (IFCIDENTIFIER)
  Graphics | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "1200x600" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "100" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "105" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "40" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "45" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "60" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "75" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "80" (IFCTEXT)
  Graphics: 2 more contents on 2 objects not shown
  Identity Data | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "standaard" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analytical Properties(Type) | properties | on 2 objects (2 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 2.6 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.384615384615385 (IFCREAL)
    Thermal mass = 420. (IFCREAL)
  Analytical Properties(Type) | properties | on 2 objects (2 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.433333333333333 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.30769230769231 (IFCREAL)
    Thermal mass = 2520. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.26 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 3.84615384615385 (IFCREAL)
    Thermal mass = 4200. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.247619047619048 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 4.03846153846154 (IFCREAL)
    Thermal mass = 4410. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.65 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.53846153846154 (IFCREAL)
    Thermal mass = 1680. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.577777777777778 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 1.73076923076923 (IFCREAL)
    Thermal mass = 1890. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.346666666666667 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 2.88461538461539 (IFCREAL)
    Thermal mass = 3150. (IFCREAL)
  Analytical Properties(Type) | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.325 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 3.07692307692308 (IFCREAL)
    Thermal mass = 3360. (IFCREAL)
  Analytical Properties(Type): 1 more content on 1 objects not shown
  Construction(Type) | properties | on 2 objects (2 IFCROOF)
    Default Thickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 2 objects (2 IFCROOF)
    Default Thickness = 60. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 105. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 40. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 45. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 75. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type) | properties | on 1 object (1 IFCROOF)
    Default Thickness = 80. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction(Type): 1 more content on 1 objects not shown
  Graphics(Type) | properties | on 11 objects (11 IFCROOF)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Text(Type) | properties | on 18 objects (18 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "BERSnl_x_rgb 0 0 0 T00 zwart_gen" (IFCLABEL)
    TBQnl_C_materiaal_02 = "BERSnl_x_rgb 255 203 012 T00 geel_gen" (IFCLABEL)

Other addresses and roles
  2 x postal address (none given)