IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-12-23T14:23:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "ktemmerman" of Organization (no name given)
  Owner history of Person "ktemmerman" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1608728402 (2020-12-23T13:00:02Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 230 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver_Recticel Insulation:92251" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver_Recticel Insulation" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          66 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "standard" | object type "BERSfr_XX_GM_FB_logo_recticel:standard" | names: "BERSfr_XX_GM_FB_logo_recticel:standard:92274", "BERSfr_XX_GM_FB_logo_recticel:standard:92293", "BERSfr_XX_GM_FB_logo_recticel:standard:92311" (+63 more) | material: materials ("BERSnl_x_rgb 0 0 0 T00 noir_gen", "RSen_x_rgb 255 203 012 T00 yellow_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          98 x IFCBUILDINGELEMENTPROXY | object type "Model Text:Model Text 1" | names: "Model Text:Model Text 1:92277", "Model Text:Model Text 1:92295", "Model Text:Model Text 1:92313" (+95 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation:92278" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x100_Recticel Insulation" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation:92296" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x100_Recticel Insulation" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation:92315" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x110_Recticel Insulation" 110.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation:92333" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x110_Recticel Insulation" 110.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation:92352" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x120_Recticel Insulation" 120.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation:92370" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x120_Recticel Insulation" 120.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation:92389" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x130_Recticel Insulation" 130.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x130_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x130_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x130_Recticel Insulation:92407" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x130_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x130_Recticel Insulation" 130.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x142_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x142_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x142_Recticel Insulation:92426" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x142_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x142_Recticel Insulation" 142.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x142_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x142_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x142_Recticel Insulation:92444" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x142_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x142_Recticel Insulation" 142.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x150_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x150_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x150_Recticel Insulation:92463" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x150_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x150_Recticel Insulation" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x150_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x150_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x150_Recticel Insulation:92481" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x150_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x150_Recticel Insulation" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x160_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x160_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x160_Recticel Insulation:92500" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x160_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x160_Recticel Insulation" 160.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x160_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x160_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x160_Recticel Insulation:92518" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x160_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x160_Recticel Insulation" 160.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x180_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x180_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x180_Recticel Insulation:92537" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x180_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x180_Recticel Insulation" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x180_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x180_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x180_Recticel Insulation:92555" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x180_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x180_Recticel Insulation" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x200_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x200_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x200_Recticel Insulation:92574" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x200_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x200_Recticel Insulation" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x200_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x200_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x200_Recticel Insulation:92592" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x200_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x200_Recticel Insulation" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x30_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x30_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x30_Recticel Insulation:92611" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x30_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x30_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x30_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x30_Recticel Insulation:92629" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x30_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x40_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x40_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x40_Recticel Insulation:92648" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x40_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x40_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x40_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x40_Recticel Insulation:92666" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x40_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x50_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x50_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x50_Recticel Insulation:92685" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x50_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x50_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x50_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x50_Recticel Insulation:92703" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x50_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x60_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x60_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x60_Recticel Insulation:92722" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x60_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x60_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x60_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x60_Recticel Insulation:92740" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x60_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x70_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x70_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x70_Recticel Insulation:92759" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x70_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x70_Recticel Insulation" 70.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x70_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x70_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x70_Recticel Insulation:92777" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x70_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x70_Recticel Insulation" 70.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x81_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x81_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x81_Recticel Insulation:92796" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x81_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x81_Recticel Insulation" 81.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x81_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x81_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x81_Recticel Insulation:92814" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x81_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x81_Recticel Insulation" 81.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x90_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x90_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x90_Recticel Insulation:92833" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x90_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x90_Recticel Insulation" 90.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x90_Recticel Insulation" | object type "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x90_Recticel Insulation" | names: "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x90_Recticel Insulation:92851" | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x90_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x90_Recticel Insulation" 90.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver_Recticel Insulation:92889" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x100_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x100_Recticel Insulation:92928" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x100_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x100_Recticel Insulation:92966" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x110_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x110_Recticel Insulation:93005" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x110_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x110_Recticel Insulation:93043" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x120_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x120_Recticel Insulation:93082" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x120_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x120_Recticel Insulation:93120" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x130_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x130_Recticel Insulation:93159" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x130_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x130_Recticel Insulation:93197" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x142_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x142_Recticel Insulation:93236" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x142_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x142_Recticel Insulation:93274" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x150_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x150_Recticel Insulation:93313" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x150_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x150_Recticel Insulation:93351" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x160_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x160_Recticel Insulation:93390" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x160_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x160_Recticel Insulation:93428" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x180_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x180_Recticel Insulation:93467" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x180_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x180_Recticel Insulation:93505" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x200_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x200_Recticel Insulation:93544" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x200_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x200_Recticel Insulation:93582" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x30_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x30_Recticel Insulation:93621" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x30_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x30_Recticel Insulation:93659" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x40_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x40_Recticel Insulation:93698" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x40_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x40_Recticel Insulation:93736" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x50_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x50_Recticel Insulation:93775" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x50_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x50_Recticel Insulation:93813" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x60_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x60_Recticel Insulation:93852" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x60_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x60_Recticel Insulation:93890" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x70_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x70_Recticel Insulation:93929" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x70_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x70_Recticel Insulation:93967" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x81_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x81_Recticel Insulation:94006" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x81_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x81_Recticel Insulation:94044" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x90_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 1200x600x90_Recticel Insulation:94083" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCROOF | object type "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x90_Recticel Insulation" | names: "Basic Roof:BERSfr_27_RO_Eurothane Silver 2400x1200x90_Recticel Insulation:94121" | parts: 1 IFCSLAB | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon

Types
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver_Recticel Insulation" 10.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "standard" | 66 occurrences | material: materials ("BERSnl_x_rgb 0 0 0 T00 noir_gen", "RSen_x_rgb 255 203 012 T00 yellow_gen") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x100_Recticel Insulation" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x100_Recticel Insulation" 100.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x110_Recticel Insulation" 110.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x110_Recticel Insulation" 110.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x120_Recticel Insulation" 120.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x120_Recticel Insulation" 120.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x130_Recticel Insulation" 130.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x130_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x130_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x130_Recticel Insulation" 130.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x142_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x142_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x142_Recticel Insulation" 142.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x142_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x142_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x142_Recticel Insulation" 142.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x150_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x150_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x150_Recticel Insulation" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x150_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x150_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x150_Recticel Insulation" 150.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x160_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x160_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x160_Recticel Insulation" 160.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x160_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x160_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x160_Recticel Insulation" 160.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x180_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x180_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x180_Recticel Insulation" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x180_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x180_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x180_Recticel Insulation" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x200_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x200_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x200_Recticel Insulation" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x200_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x200_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x200_Recticel Insulation" 200.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x30_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x30_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x30_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x30_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x30_Recticel Insulation" 30.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x40_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x40_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x40_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x40_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x40_Recticel Insulation" 40.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x50_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x50_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x50_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x50_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x50_Recticel Insulation" 50.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x60_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x60_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x60_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x60_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x60_Recticel Insulation" 60.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x70_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x70_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x70_Recticel Insulation" 70.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x70_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x70_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x70_Recticel Insulation" 70.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x81_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x81_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x81_Recticel Insulation" 81.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x81_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x81_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x81_Recticel Insulation" 81.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x90_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 1200x600x90_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 1200x600x90_Recticel Insulation" 90.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x90_Recticel Insulation" | STANDARD | 1 occurrence | material: layers "Basic Wall:BERSfr_22_WA_Eurothane Silver 2400x1200x90_Recticel Insulation" ("BERSfr_MFS.n7_isolation_Eurothane Silver 2400x1200x90_Recticel Insulation" 90.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Property sets
  Pset_ElementShading | properties | on 99 objects (33 IFCROOF, 33 IFCSLAB, 33 IFCWALLSTANDARDCASE) | on 33 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 164 objects (164 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 66 objects (33 IFCROOF, 33 IFCSLAB)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 33 objects (33 IFCWALLSTANDARDCASE) | on 33 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 98 objects (98 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 66 objects (66 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x110_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCROOF, 1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 60 more contents on 87 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 25 more contents on 25 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 2400x1200x110_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 2400x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "BERSfr_22_WA_Eurothane Silver 1200x600x130_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.169230769230769 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 58 more contents on 25 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 98 objects (98 IFCBUILDINGELEMENTPROXY)
    Reference = "Model Text 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 66 objects (66 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "standard" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x110_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x130_Recticel Insulation" (IFCIDENTIFIER)
    TotalArea = 11.24126784 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon: 25 more contents on 25 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x100_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x110_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x110_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x120_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x130_Recticel Insulation" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 25 more contents on 25 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 2.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x100_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.22 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x110_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x110_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 2400x1200x120_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.183333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "BERSfr_27_RO_Eurothane Silver 1200x600x130_Recticel Insulation" (IFCIDENTIFIER)
    ThermalTransmittance = 0.169230769230769 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 25 more contents on 25 objects not shown
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)

Other addresses and roles
  2 x postal address (none given)